# Float message from three infrared sensors IO pin.
std_msgs/Header header

uint8 INFRARED=1
uint8 radiation_type

float32 field_of_view
float32 min_range
float32 max_range

float32 front_dist
float32 left_dist
float32 right_dist
